(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "USLetter")
  (title_block
    (title "Rovotron Top Board")
    (rev "C")
    (company "Cathode Corner")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010e0_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "+5V")
  (net 3 "/SERA")
  (net 4 "/SERB")
  (net 5 "/VID+")
  (net 6 "/VID-")
  (net 7 "/RXD")
  (net 8 "/RXD5")
  (net 9 "/TXD")
  (net 10 "/TXE")
  (net 11 "/USB_VBUS")
  (net 12 "/USB_D-")
  (net 13 "/USB_D+")
  (net 14 "/DISP_D4")
  (net 15 "/DISP_D5")
  (net 16 "/DISP_D6")
  (net 17 "/DISP_D7")
  (net 18 "unconnected-(M1-DB0-Pad7)")
  (net 19 "/CONT")
  (net 20 "unconnected-(M1-DB1-Pad8)")
  (net 21 "/DISP_RS")
  (net 22 "unconnected-(M1-DB2-Pad9)")
  (net 23 "/DISP_RW")
  (net 24 "unconnected-(M1-DB3-Pad10)")
  (net 25 "/DISP_E")
  (net 26 "/VID")
  (net 27 "/VID_RET")
  (net 28 "Net-(M1-DB4)")
  (net 29 "Net-(M1-DB5)")
  (net 30 "Net-(M1-DB6)")
  (net 31 "Net-(M1-DB7)")
  (net 32 "Net-(R10-Pad2)")
  (net 33 "/12V")
  (net 34 "/AUD+")
  (net 35 "/AUD-")
  (net 36 "unconnected-(M2-3_LRCLK2-Pad5)")
  (net 37 "unconnected-(M2-4_BCLK2-Pad6)")
  (net 38 "unconnected-(M2-8_TX2_IN1-Pad10)")
  (net 39 "unconnected-(M2-9_OUT1C-Pad11)")
  (net 40 "unconnected-(M2-10_CS_MQSR-Pad12)")
  (net 41 "unconnected-(M2-11_MOSI_CTX1-Pad13)")
  (net 42 "unconnected-(M2-12_MISO_MQSL-Pad14)")
  (net 43 "unconnected-(M2-3V3-Pad15)")
  (net 44 "unconnected-(M2-28_RX7-Pad20)")
  (net 45 "unconnected-(M2-29_TX7-Pad21)")
  (net 46 "unconnected-(M2-30_CRX3-Pad22)")
  (net 47 "unconnected-(M2-31_CTX3-Pad23)")
  (net 48 "unconnected-(M2-32_OUT1B-Pad24)")
  (net 49 "unconnected-(M2-33_MCLK2-Pad25)")
  (net 50 "unconnected-(M2-34_RX8-Pad26)")
  (net 51 "unconnected-(M2-35_TX8-Pad27)")
  (net 52 "unconnected-(M2-36_CS-Pad28)")
  (net 53 "unconnected-(M2-37_CS-Pad29)")
  (net 54 "unconnected-(M2-38_CS1_IN1-Pad30)")
  (net 55 "unconnected-(M2-39_MISO1_OUT1A-Pad31)")
  (net 56 "unconnected-(M2-40_A16-Pad32)")
  (net 57 "unconnected-(M2-41_A17-Pad33)")
  (net 58 "unconnected-(M2-13_SCK_LED-Pad35)")
  (net 59 "unconnected-(M2-14_A0_TX3_SPDIF_OUT-Pad36)")
  (net 60 "unconnected-(M2-15_A1_RX3_SPDIF_IN-Pad37)")
  (net 61 "unconnected-(M2-16_A2_RX4_SCL1-Pad38)")
  (net 62 "unconnected-(M2-17_A3_TX4_SDA1-Pad39)")
  (net 63 "unconnected-(M2-18_A4_SDA-Pad40)")
  (net 64 "unconnected-(M2-19_A5_SCL-Pad41)")
  (net 65 "unconnected-(M2-20_A6_TX5_LRCLK1-Pad42)")
  (net 66 "unconnected-(M2-21_A7_RX5_BCLK1-Pad43)")
  (net 67 "unconnected-(M2-22_A8_CTX1-Pad44)")
  (net 68 "unconnected-(M2-23_A9_CRX1_MCLK1-Pad45)")
  (net 69 "unconnected-(M2-3V3-Pad46)")
  (footprint "Capacitor_THT:CP_Radial_D10.0mm_P3.50mm" (layer "F.Cu")
    (at 113.03 45.72 90)
    (descr "CP, Radial series, Radial, pin pitch=3.50mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 3.50mm  diameter 10mm Electrolytic Capacitor")
    (property "Sheetfile" "RVTOP-C.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor, US symbol")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C3" (at -0.635 -6.35 180) (layer "F.SilkS"))
    (fp_text value "470uF25V" (at 1.75 6.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.75 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 33 "/12V") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5 0 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P3.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 152.4 38.1 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "RVTOP-C.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R9" (at 12.7 0 -180) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(M1-DB7)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 17 "/DISP_D7") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Rovo:Transformer_Balun_Board" (layer "F.Cu")
    (at 119.38 73 180)
    (descr "Balun board from BNC to screw terminal (removed from Amazon unit)")
    (tags "Transformer Toroid balun video")
    (property "Sheetfile" "RVTOP-C.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Transformer, Balun, Video, Simonsen123 344E")
    (attr through_hole)
    (fp_text reference "T1" (at 0 7) (layer "F.SilkS"))
    (fp_text value "Balun" (at -0.762 6.858) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 7.112 -3.556 180) (size 3.048 3.048) (drill 1.778) (layers "*.Cu" "*.Mask")
      (net 26 "/VID") (pinfunction "VidSig") (pintype "passive"))
    (pad "2" thru_hole circle (at 7.112 3.556 180) (size 3.048 3.048) (drill 1.778) (layers "*.Cu" "*.Mask")
      (net 27 "/VID_RET") (pinfunction "VidRet") (pintype "passive"))
    (pad "3" thru_hole circle (at -10.668 2.54 180) (size 3.048 3.048) (drill 1.778) (layers "*.Cu" "*.Mask")
      (net 6 "/VID-") (pinfunction "Vid-") (pintype "passive"))
    (pad "4" thru_hole circle (at -10.668 -2.54 180) (size 3.048 3.048) (drill 1.778) (layers "*.Cu" "*.Mask")
      (net 5 "/VID+") (pinfunction "Vid+") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 -3.556 180) (size 3.048 3.048) (drill 1.778) (layers "*.Cu" "*.Mask"))
    (pad "6" thru_hole circle (at 0 0 180) (size 2.54 2.54) (drill 1.27) (layers "*.Cu" "*.Mask"))
    (pad "7" thru_hole circle (at 0 3.556 180) (size 3.048 3.048) (drill 1.778) (layers "*.Cu" "*.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/Transformer_THT.3dshapes/Transformer_Toroid_Horizontal_D12.5mm_Amidon-T44.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_USB:USB_A_Molex_67643_Horizontal" (layer "F.Cu")
    (at 162.56 78.74)
    (descr "USB type A, Horizontal, https://www.molex.com/pdm_docs/sd/676433910_sd.pdf")
    (tags "USB_A Female Connector receptacle")
    (property "Sheetfile" "RVTOP-C.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "USB Type A connector")
    (property "ki_keywords" "connector USB")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -3.81) (layer "F.SilkS"))
    (fp_text value "Gamepad" (at 5.08 -3.81) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.5 3.7) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.5) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 11 "/USB_VBUS") (pinfunction "VBUS") (pintype "power_in"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 12 "/USB_D-") (pinfunction "D-") (pintype "bidirectional"))
    (pad "3" thru_hole circle (at 4.5 0) (size 1.6 1.6) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 13 "/USB_D+") (pinfunction "D+") (pintype "bidirectional"))
    (pad "4" thru_hole circle (at 7 0) (size 1.6 1.6) (drill 0.95) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole circle (at -3.07 2.71) (size 3 3) (drill 2.3) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "5" thru_hole circle (at 10.07 2.71) (size 3 3) (drill 2.3) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_USB.3dshapes/USB_A_Molex_67643_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Rovo:NHD_0420DZ" locked (layer "F.Cu")
    (at 111 32.5)
    (descr "STN/FSTN LCD 192x64 dot https://www.buydisplay.com/download/manual/ERM19264-1_Series_Datasheet.pdf")
    (tags "ERM19264 Graphics Display 192x64")
    (property "Sheetfile" "RVTOP-C.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "LCD 20x4 Alphanumeric 16pin Blue/White/Green Backlight, 8bit parallel")
    (property "ki_keywords" "display LCD 20x4")
    (attr through_hole)
    (fp_text reference "M1" (at -1.78 3.06) (layer "F.SilkS"))
    (fp_text value "NHD-0420DZ" (at -1 60) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 21.5 6.5) (layer "F.Fab"))
    (pad "" thru_hole circle locked (at -7.5 0 180) (size 5 5) (drill 2.5) (layers "*.Cu" "*.Mask"))
    (pad "" thru_hole circle locked (at -7.5 55 180) (size 5 5) (drill 2.5) (layers "*.Cu" "*.Mask"))
    (pad "" thru_hole circle locked (at 85.5 0 180) (size 5 5) (drill 2.5) (layers "*.Cu" "*.Mask"))
    (pad "" thru_hole circle locked (at 85.5 55 180) (size 5 5) (drill 2.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.8 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "2" thru_hole oval locked (at 2.54 0 180) (size 1.8 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 2 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "3" thru_hole oval locked (at 5.08 0 180) (size 1.8 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 19 "/CONT") (pinfunction "VO") (pintype "power_in"))
    (pad "4" thru_hole oval locked (at 7.62 0 180) (size 1.8 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 21 "/DISP_RS") (pinfunction "RS") (pintype "input"))
    (pad "5" thru_hole oval locked (at 10.16 0 180) (size 1.8 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 23 "/DISP_RW") (pinfunction "R/W") (pintype "input"))
    (pad "6" thru_hole oval locked (at 12.7 0 180) (size 1.8 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 25 "/DISP_E") (pinfunction "E") (pintype "input"))
    (pad "7" thru_hole oval locked (at 15.24 0 180) (size 1.8 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 18 "unconnected-(M1-DB0-Pad7)") (pinfunction "DB0") (pintype "bidirectional"))
    (pad "8" thru_hole oval locked (at 17.78 0 180) (size 1.8 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 20 "unconnected-(M1-DB1-Pad8)") (pinfunction "DB1") (pintype "bidirectional"))
    (pad "9" thru_hole oval locked (at 20.32 0 180) (size 1.8 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 22 "unconnected-(M1-DB2-Pad9)") (pinfunction "DB2") (pintype "bidirectional"))
    (pad "10" thru_hole oval locked (at 22.86 0 180) (size 1.8 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 24 "unconnected-(M1-DB3-Pad10)") (pinfunction "DB3") (pintype "bidirectional"))
    (pad "11" thru_hole oval locked (at 25.4 0 180) (size 1.8 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(M1-DB4)") (pinfunction "DB4") (pintype "bidirectional"))
    (pad "12" thru_hole oval locked (at 27.94 0 180) (size 1.8 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(M1-DB5)") (pinfunction "DB5") (pintype "bidirectional"))
    (pad "13" thru_hole oval locked (at 30.48 0 180) (size 1.8 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 30 "Net-(M1-DB6)") (pinfunction "DB6") (pintype "bidirectional"))
    (pad "14" thru_hole oval locked (at 33.02 0 180) (size 1.8 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(M1-DB7)") (pinfunction "DB7") (pintype "bidirectional"))
    (pad "15" thru_hole oval locked (at 35.56 0 180) (size 1.8 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 2 "+5V") (pinfunction "LED+") (pintype "passive"))
    (pad "16" thru_hole oval locked (at 38.1 0 180) (size 1.8 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "LED-") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Display.3dshapes/ERM19264.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D10.0mm_P3.50mm" (layer "F.Cu")
    (at 124.46 45.72 90)
    (descr "CP, Radial series, Radial, pin pitch=3.50mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 3.50mm  diameter 10mm Electrolytic Capacitor")
    (property "Sheetfile" "RVTOP-C.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor, US symbol")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C4" (at -0.635 6.35 180) (layer "F.SilkS"))
    (fp_text value "470uF25V" (at 1.75 6.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.75 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5 0 90) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P3.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Potentiometer_Bourns_3386X_Horizontal" (layer "F.Cu")
    (at 104.775 62.23 180)
    (descr "Potentiometer, horizontal, Bourns 3386X, https://www.bourns.com/pdfs/3386.pdf")
    (tags "Potentiometer horizontal Bourns 3386X")
    (property "Sheetfile" "RVTOP-C.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer")
    (property "ki_keywords" "resistor variable")
    (attr through_hole)
    (fp_text reference "RV1" (at 1.27 -3.81) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 8.555) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2.54) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.44 1.44) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(R10-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 2.54 180) (size 1.44 1.44) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "/CONT") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5.08 180) (size 1.44 1.44) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3386X_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Rovo:Teensy41_48_5" (layer "F.Cu")
    (at 184.15 59.69 90)
    (property "Sheetfile" "RVTOP-C.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "M2" (at -21.59 10.795 180) (layer "F.SilkS"))
    (fp_text value "Teensy4.1" (at 0 10.16 90) (layer "F.Fab"))
    (fp_text user "USB Host" (at -18.4658 2.4892 90) (layer "F.SilkS"))
    (fp_text user "MIMXRT1062" (at -1.27 0) (layer "F.SilkS"))
    (fp_text user "USB" (at -26.67 0) (layer "F.SilkS"))
    (fp_text user "Micro SD" (at 24.13 0 90) (layer "F.SilkS"))
    (fp_text user "DVJ6A" (at -2.54 -0.18) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -29.21 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" thru_hole circle (at -26.67 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 7 "/RXD") (pinfunction "0_RX1_CRX2_CS1") (pintype "bidirectional"))
    (pad "3" thru_hole circle (at -24.13 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 9 "/TXD") (pinfunction "1_TX1_CTX2_MISO1") (pintype "bidirectional"))
    (pad "4" thru_hole circle (at -21.59 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 10 "/TXE") (pinfunction "2_OUT2") (pintype "bidirectional"))
    (pad "5" thru_hole circle (at -19.05 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 36 "unconnected-(M2-3_LRCLK2-Pad5)") (pinfunction "3_LRCLK2") (pintype "bidirectional"))
    (pad "6" thru_hole circle (at -16.51 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 37 "unconnected-(M2-4_BCLK2-Pad6)") (pinfunction "4_BCLK2") (pintype "bidirectional"))
    (pad "7" thru_hole circle (at -13.97 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 21 "/DISP_RS") (pinfunction "5_IN2") (pintype "bidirectional"))
    (pad "8" thru_hole circle (at -11.43 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 23 "/DISP_RW") (pinfunction "6_OUT1D") (pintype "bidirectional"))
    (pad "9" thru_hole circle (at -8.89 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 25 "/DISP_E") (pinfunction "7_RX2_OUT1A") (pintype "bidirectional"))
    (pad "10" thru_hole circle (at -6.35 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 38 "unconnected-(M2-8_TX2_IN1-Pad10)") (pinfunction "8_TX2_IN1") (pintype "bidirectional"))
    (pad "11" thru_hole circle (at -3.81 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 39 "unconnected-(M2-9_OUT1C-Pad11)") (pinfunction "9_OUT1C") (pintype "bidirectional"))
    (pad "12" thru_hole circle (at -1.27 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 40 "unconnected-(M2-10_CS_MQSR-Pad12)") (pinfunction "10_CS_MQSR") (pintype "bidirectional"))
    (pad "13" thru_hole circle (at 1.27 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 41 "unconnected-(M2-11_MOSI_CTX1-Pad13)") (pinfunction "11_MOSI_CTX1") (pintype "bidirectional"))
    (pad "14" thru_hole circle (at 3.81 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 42 "unconnected-(M2-12_MISO_MQSL-Pad14)") (pinfunction "12_MISO_MQSL") (pintype "bidirectional"))
    (pad "15" thru_hole circle (at 6.35 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 43 "unconnected-(M2-3V3-Pad15)") (pinfunction "3V3") (pintype "power_in"))
    (pad "16" thru_hole circle (at 8.89 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 14 "/DISP_D4") (pinfunction "24_A10_TX6_SCL2") (pintype "bidirectional"))
    (pad "17" thru_hole circle (at 11.43 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 15 "/DISP_D5") (pinfunction "25_A11_RX6_SDA2") (pintype "bidirectional"))
    (pad "18" thru_hole circle (at 13.97 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 16 "/DISP_D6") (pinfunction "26_A12_MOSI1") (pintype "bidirectional"))
    (pad "19" thru_hole circle (at 16.51 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 17 "/DISP_D7") (pinfunction "27_A13_SCK1") (pintype "bidirectional"))
    (pad "20" thru_hole circle (at 19.05 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 44 "unconnected-(M2-28_RX7-Pad20)") (pinfunction "28_RX7") (pintype "bidirectional"))
    (pad "21" thru_hole circle (at 21.59 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 45 "unconnected-(M2-29_TX7-Pad21)") (pinfunction "29_TX7") (pintype "bidirectional"))
    (pad "22" thru_hole circle (at 24.13 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 46 "unconnected-(M2-30_CRX3-Pad22)") (pinfunction "30_CRX3") (pintype "bidirectional"))
    (pad "23" thru_hole circle (at 26.67 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 47 "unconnected-(M2-31_CTX3-Pad23)") (pinfunction "31_CTX3") (pintype "bidirectional"))
    (pad "24" thru_hole circle (at 29.21 7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 48 "unconnected-(M2-32_OUT1B-Pad24)") (pinfunction "32_OUT1B") (pintype "bidirectional"))
    (pad "25" thru_hole circle (at 29.21 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 49 "unconnected-(M2-33_MCLK2-Pad25)") (pinfunction "33_MCLK2") (pintype "bidirectional"))
    (pad "26" thru_hole circle (at 26.67 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 50 "unconnected-(M2-34_RX8-Pad26)") (pinfunction "34_RX8") (pintype "bidirectional"))
    (pad "27" thru_hole circle (at 24.13 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 51 "unconnected-(M2-35_TX8-Pad27)") (pinfunction "35_TX8") (pintype "bidirectional"))
    (pad "28" thru_hole circle (at 21.59 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 52 "unconnected-(M2-36_CS-Pad28)") (pinfunction "36_CS") (pintype "bidirectional"))
    (pad "29" thru_hole circle (at 19.05 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 53 "unconnected-(M2-37_CS-Pad29)") (pinfunction "37_CS") (pintype "bidirectional"))
    (pad "30" thru_hole circle (at 16.51 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 54 "unconnected-(M2-38_CS1_IN1-Pad30)") (pinfunction "38_CS1_IN1") (pintype "bidirectional"))
    (pad "31" thru_hole circle (at 13.97 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 55 "unconnected-(M2-39_MISO1_OUT1A-Pad31)") (pinfunction "39_MISO1_OUT1A") (pintype "bidirectional"))
    (pad "32" thru_hole circle (at 11.43 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 56 "unconnected-(M2-40_A16-Pad32)") (pinfunction "40_A16") (pintype "bidirectional"))
    (pad "33" thru_hole circle (at 8.89 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 57 "unconnected-(M2-41_A17-Pad33)") (pinfunction "41_A17") (pintype "bidirectional"))
    (pad "34" thru_hole circle (at 6.35 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "35" thru_hole circle (at 3.81 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 58 "unconnected-(M2-13_SCK_LED-Pad35)") (pinfunction "13_SCK_LED") (pintype "bidirectional"))
    (pad "36" thru_hole circle (at 1.27 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 59 "unconnected-(M2-14_A0_TX3_SPDIF_OUT-Pad36)") (pinfunction "14_A0_TX3_SPDIF_OUT") (pintype "bidirectional"))
    (pad "37" thru_hole circle (at -1.27 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 60 "unconnected-(M2-15_A1_RX3_SPDIF_IN-Pad37)") (pinfunction "15_A1_RX3_SPDIF_IN") (pintype "bidirectional"))
    (pad "38" thru_hole circle (at -3.81 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 61 "unconnected-(M2-16_A2_RX4_SCL1-Pad38)") (pinfunction "16_A2_RX4_SCL1") (pintype "bidirectional"))
    (pad "39" thru_hole circle (at -6.35 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 62 "unconnected-(M2-17_A3_TX4_SDA1-Pad39)") (pinfunction "17_A3_TX4_SDA1") (pintype "bidirectional"))
    (pad "40" thru_hole circle (at -8.89 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 63 "unconnected-(M2-18_A4_SDA-Pad40)") (pinfunction "18_A4_SDA") (pintype "bidirectional"))
    (pad "41" thru_hole circle (at -11.43 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 64 "unconnected-(M2-19_A5_SCL-Pad41)") (pinfunction "19_A5_SCL") (pintype "bidirectional"))
    (pad "42" thru_hole circle (at -13.97 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 65 "unconnected-(M2-20_A6_TX5_LRCLK1-Pad42)") (pinfunction "20_A6_TX5_LRCLK1") (pintype "bidirectional"))
    (pad "43" thru_hole circle (at -16.51 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 66 "unconnected-(M2-21_A7_RX5_BCLK1-Pad43)") (pinfunction "21_A7_RX5_BCLK1") (pintype "bidirectional"))
    (pad "44" thru_hole circle (at -19.05 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 67 "unconnected-(M2-22_A8_CTX1-Pad44)") (pinfunction "22_A8_CTX1") (pintype "bidirectional"))
    (pad "45" thru_hole circle (at -21.59 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 68 "unconnected-(M2-23_A9_CRX1_MCLK1-Pad45)") (pinfunction "23_A9_CRX1_MCLK1") (pintype "bidirectional"))
    (pad "46" thru_hole circle (at -24.13 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 69 "unconnected-(M2-3V3-Pad46)") (pinfunction "3V3") (pintype "output"))
    (pad "47" thru_hole circle (at -26.67 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "output"))
    (pad "48" thru_hole circle (at -29.21 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "+5V") (pinfunction "VIN") (pintype "power_in"))
    (pad "49" thru_hole rect (at -22.9108 4.5692 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 11 "/USB_VBUS") (pinfunction "5V") (pintype "power_out"))
    (pad "50" thru_hole circle (at -20.3708 4.5692 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 12 "/USB_D-") (pinfunction "D-") (pintype "bidirectional"))
    (pad "51" thru_hole circle (at -17.8308 4.5692 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 13 "/USB_D+") (pinfunction "D+") (pintype "bidirectional"))
    (pad "52" thru_hole circle (at -15.2908 4.5692 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "53" thru_hole circle (at -12.7508 4.5692 90) (size 1.6 1.6) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (model "${KICAD_USER_DIR}/teensy.pretty/Teensy_4.1_Assembly.STEP"
      (offset (xyz 0 0 0.762))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-8_W7.62mm" (layer "F.Cu")
    (at 167.64 66.04 180)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Category" "Integrated Circuits (ICs)")
    (property "DK_Datasheet_Link" "http://www.ti.com/general/docs/suppproductinfo.tsp?distId=10&gotoUrl=http%3A%2F%2Fwww.ti.com%2Flit%2Fgpn%2Fsn65176b")
    (property "DK_Detail_Page" "/product-detail/en/texas-instruments/SN75176BDR/296-1275-1-ND/404925")
    (property "Description" "IC TXRX DIFF BUSS 8SOIC")
    (property "Digi-Key_PN" "296-17498-5-ND")
    (property "Family" "Interface - Drivers, Receivers, Transceivers")
    (property "MPN" "SN65HVD485EP")
    (property "Manufacturer" "Texas Instruments")
    (property "Sheetfile" "RVTOP-C.kicad_sch")
    (property "Sheetname" "")
    (property "Status" "Active")
    (property "ki_description" "IC TXRX DIFF BUSS 8SOIC")
    (property "ki_keywords" "296-1275-1-ND")
    (attr through_hole)
    (fp_text reference "U2" (at -2.54 0 180) (layer "F.SilkS"))
    (fp_text value "SN65HVD485EP" (at 3.81 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "/RXD5") (pinfunction "R") (pintype "output"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "/TXE") (pinfunction "~{RE}") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "/TXE") (pinfunction "DE") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "/TXD") (pinfunction "D") (pintype "input"))
    (pad "5" thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "6" thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "/SERA") (pinfunction "A") (pintype "bidirectional"))
    (pad "7" thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "/SERB") (pinfunction "B") (pintype "bidirectional"))
    (pad "8" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Rovo:Connector_CUI_RCJ_01_Horizontal" (layer "F.Cu")
    (at 132.08 85.09 180)
    (descr "CUI RCJ-01 horizontal")
    (tags "Phono RCA coaxial jack")
    (property "Sheetfile" "RVTOP-C.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA")
    (attr through_hole)
    (fp_text reference "J3" (at 0 3.5) (layer "F.SilkS"))
    (fp_text value "AUDIO" (at 0 5.08) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 3 3) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 34 "/AUD+") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at -5 0 180) (size 4 4) (drill 2.6) (layers "*.Cu" "*.Mask")
      (net 35 "/AUD-") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 -4.5 180) (size 4 4) (drill 2.6) (layers "*.Cu" "*.Mask")
      (net 35 "/AUD-") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 4 4) (drill 2.6) (layers "*.Cu" "*.Mask")
      (net 35 "/AUD-") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/BNC_TEConnectivity_1478035_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 180.34 83.82 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "RVTOP-C.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R2" (at 12.7 0) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "/RXD") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "/RXD5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT" (layer "F.Cu")
    (at 119.38 58.42)
    (descr "DCDC-Converter, RECOM, RECOM_R-78E-0.5, SIP-3, pitch 2.54mm, package size 11.6x8.5x10.4mm^3, https://www.recom-power.com/pdf/Innoline/R-78Exx-0.5.pdf")
    (tags "dc-dc recom buck sip-3 pitch 2.54mm")
    (property "Sheetfile" "RVTOP-C.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "1A Step-Down DC/DC-Regulator, 7-28V input, 5V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3")
    (property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator")
    (attr through_hole)
    (fp_text reference "U4" (at 0.067 4.1825 180) (layer "F.SilkS"))
    (fp_text value "R-78E5.0-1.0" (at 2.54 3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -2.25) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.5 2.3) (drill 1) (layers "*.Cu" "*.Mask")
      (net 33 "/12V") (pinfunction "IN") (pintype "power_in"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.5 2.3) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval (at 5.08 0) (size 1.5 2.3) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "+5V") (pinfunction "OUT") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Converter_DCDC.3dshapes/Converter_DCDC_RECOM_R-78E-0.5_THT.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02" (layer "F.Cu")
    (at 162.56 69.85)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4.6*2mm^2, Capacitor, http://www.wima.de/DE/WIMA_MKS_02.pdf")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4.6mm width 2mm Capacitor")
    (property "Sheetfile" "RVTOP-C.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at 5.08 0 180) (layer "F.SilkS"))
    (fp_text value "0.1uF_50V_X7R_Rad" (at 1.25 2.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 144.78 38.1 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "RVTOP-C.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R7" (at 12.7 0 -180) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(M1-DB5)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "/DISP_D5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 183.515 83.82 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "RVTOP-C.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R3" (at 12.7 0 180) (layer "F.SilkS"))
    (fp_text value "2K" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "/RXD") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 147.32 66.04 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "RVTOP-C.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R4" (at -2.54 0) (layer "F.SilkS"))
    (fp_text value "10K" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "+5V") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "/SERA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_RJ:RJ45_Amphenol_54602-x08_Horizontal" (layer "F.Cu")
    (at 144.145 77.47)
    (descr "8 Pol Shallow Latch Connector, Modjack, RJ45 (https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/c-bmj-0102.pdf)")
    (tags "RJ45")
    (property "Sheetfile" "RVTOP-C.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RJ connector, 8P8C (8 positions 8 connected), RJ31/RJ32/RJ33/RJ34/RJ35/RJ41/RJ45/RJ49/RJ61")
    (property "ki_keywords" "8P8C RJ socket connector")
    (attr through_hole)
    (fp_text reference "J4" (at 1.27 -5.08) (layer "F.SilkS"))
    (fp_text value "Tether" (at 7.62 -5.08) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.445 2) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -1.27 6.35) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 10.16 6.35) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at 0 0) (size 1.5 1.5) (drill 0.76) (layers "*.Cu" "*.Mask")
      (net 5 "/VID+") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.27 -2.54) (size 1.5 1.5) (drill 0.76) (layers "*.Cu" "*.Mask")
      (net 6 "/VID-") (pintype "passive"))
    (pad "3" thru_hole circle (at 2.54 0) (size 1.5 1.5) (drill 0.76) (layers "*.Cu" "*.Mask")
      (net 4 "/SERB") (pintype "passive"))
    (pad "4" thru_hole circle (at 3.81 -2.54) (size 1.5 1.5) (drill 0.76) (layers "*.Cu" "*.Mask")
      (net 33 "/12V") (pintype "passive"))
    (pad "5" thru_hole circle (at 5.08 0) (size 1.5 1.5) (drill 0.76) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "6" thru_hole circle (at 6.35 -2.54) (size 1.5 1.5) (drill 0.76) (layers "*.Cu" "*.Mask")
      (net 3 "/SERA") (pintype "passive"))
    (pad "7" thru_hole circle (at 7.62 0) (size 1.5 1.5) (drill 0.76) (layers "*.Cu" "*.Mask")
      (net 34 "/AUD+") (pintype "passive"))
    (pad "8" thru_hole circle (at 8.89 -2.54) (size 1.5 1.5) (drill 0.76) (layers "*.Cu" "*.Mask")
      (net 35 "/AUD-") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_RJ.3dshapes/RJ45_Amphenol_54602-x08_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Rovo:Connector_CUI_RCJ_01_Horizontal" (layer "F.Cu")
    (at 114.935 85.09 180)
    (descr "CUI RCJ-01 horizontal")
    (tags "Phono RCA coaxial jack")
    (property "Sheetfile" "RVTOP-C.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA")
    (attr through_hole)
    (fp_text reference "J2" (at 0 3.5) (layer "F.SilkS"))
    (fp_text value "VIDEO" (at 0 5) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 3 3) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 26 "/VID") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at -5 0 180) (size 4 4) (drill 2.6) (layers "*.Cu" "*.Mask")
      (net 27 "/VID_RET") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 -4.5 180) (size 4 4) (drill 2.6) (layers "*.Cu" "*.Mask")
      (net 27 "/VID_RET") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 4 4) (drill 2.6) (layers "*.Cu" "*.Mask")
      (net 27 "/VID_RET") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/BNC_TEConnectivity_1478035_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 154.94 55.88 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "RVTOP-C.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R5" (at 12.7 0 -180) (layer "F.SilkS"))
    (fp_text value "10K" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "/SERB") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 151.13 55.88 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "RVTOP-C.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R1" (at 12.7 0 -180) (layer "F.SilkS"))
    (fp_text value "100Ohm" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "/SERA") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "/SERB") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 148.59 38.1 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "RVTOP-C.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R8" (at 12.7 0 -180) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 30 "Net-(M1-DB6)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "/DISP_D6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 140.97 38.1 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "RVTOP-C.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R6" (at 12.7 0 -180) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(M1-DB4)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "/DISP_D4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (at 110.49 51.435 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "RVTOP-C.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R10" (at 12.7 0) (layer "F.SilkS"))
    (fp_text value "2K" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "+5V") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(R10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 99.06 27.94) (end 200.66 92.075)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "RVTOP-C" (at 155.575 37.465) (layer "F.SilkS"))
  (gr_text "(C)2024 David Forbes" (at 196.215 43.815 270) (layer "F.SilkS"))
  (gr_text "Rovotron" (at 156.21 33.02) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.254))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.381) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 99.695 28.575)
        (xy 200.025 28.575)
        (xy 200.025 91.44)
        (xy 99.695 91.44)
      )
    )
  )
)
