(kicad_sch (version 20230121) (generator eeschema)
  (paper "A")
  (title_block
    (title "Rovotron Top Board")
    (date "2024-01-23")
    (rev "C")
    (company "Cathode Corner")
  )
  (lib_symbols
    (symbol "Connector:8P8C" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "J" (at -5.08 13.97 0))
      (property "Value" "8P8C" (at 2.54 13.97 0))
      (property "Footprint" "" (at 0 0.635 90))
      (property "Datasheet" "~" (at 0 0.635 90))
      (property "ki_keywords" "8P8C RJ socket connector" (at 0 0 0))
      (property "ki_description" "RJ connector, 8P8C (8 positions 8 connected), RJ31/RJ32/RJ33/RJ34/RJ35/RJ41/RJ45/RJ49/RJ61" (at 0 0 0))
      (property "ki_fp_filters" "8P8C* RJ31* RJ32* RJ33* RJ34* RJ35* RJ41* RJ45* RJ49* RJ61*" (at 0 0 0))
      (symbol "8P8C_0_1"
        (polyline
          (pts
            (xy -5.08 4.445)
            (xy -6.35 4.445)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 5.715)
            (xy -6.35 5.715)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -6.35 -3.175)
            (xy -5.08 -3.175)
            (xy -5.08 -3.175)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -6.35 -1.905)
            (xy -5.08 -1.905)
            (xy -5.08 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -6.35 -0.635)
            (xy -5.08 -0.635)
            (xy -5.08 -0.635)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -6.35 0.635)
            (xy -5.08 0.635)
            (xy -5.08 0.635)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -6.35 1.905)
            (xy -5.08 1.905)
            (xy -5.08 1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 3.175)
            (xy -6.35 3.175)
            (xy -6.35 3.175)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -6.35 -4.445)
            (xy -6.35 6.985)
            (xy 3.81 6.985)
            (xy 3.81 4.445)
            (xy 5.08 4.445)
            (xy 5.08 3.175)
            (xy 6.35 3.175)
            (xy 6.35 -0.635)
            (xy 5.08 -0.635)
            (xy 5.08 -1.905)
            (xy 3.81 -1.905)
            (xy 3.81 -4.445)
            (xy -6.35 -4.445)
            (xy -6.35 -4.445)
          )
          (fill (type none))
        )
        (rectangle (start 7.62 12.7) (end -7.62 -10.16)
          (fill (type background))
        )
      )
      (symbol "8P8C_1_1"
        (pin passive line (at 10.16 -7.62 180) (length 2.54)
          (name "~")
          (number "1")
        )
        (pin passive line (at 10.16 -5.08 180) (length 2.54)
          (name "~")
          (number "2")
        )
        (pin passive line (at 10.16 -2.54 180) (length 2.54)
          (name "~")
          (number "3")
        )
        (pin passive line (at 10.16 0 180) (length 2.54)
          (name "~")
          (number "4")
        )
        (pin passive line (at 10.16 2.54 180) (length 2.54)
          (name "~")
          (number "5")
        )
        (pin passive line (at 10.16 5.08 180) (length 2.54)
          (name "~")
          (number "6")
        )
        (pin passive line (at 10.16 7.62 180) (length 2.54)
          (name "~")
          (number "7")
        )
        (pin passive line (at 10.16 10.16 180) (length 2.54)
          (name "~")
          (number "8")
        )
      )
    )
    (symbol "Connector:Conn_Coaxial" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (at 0.254 3.048 0))
      (property "Value" "Conn_Coaxial" (at 2.921 0 90))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" " ~" (at 0 0 0))
      (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA" (at 0 0 0))
      (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)" (at 0 0 0))
      (property "ki_fp_filters" "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO*" (at 0 0 0))
      (symbol "Conn_Coaxial_0_1"
        (arc (start -1.778 -0.508) (mid 0.2311 -1.8066) (end 1.778 0)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 0)
            (xy -0.508 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -2.54)
            (xy 0 -1.778)
          )
          (fill (type none))
        )
        (circle (center 0 0) (radius 0.508)
          (fill (type none))
        )
        (arc (start 1.778 0) (mid 0.2099 1.8101) (end -1.778 0.508)
          (fill (type none))
        )
      )
      (symbol "Conn_Coaxial_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "In")
          (number "1")
        )
        (pin passive line (at 0 -5.08 90) (length 2.54)
          (name "Ext")
          (number "2")
        )
      )
    )
    (symbol "Connector:USB_A" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "J" (at -5.08 11.43 0))
      (property "Value" "USB_A" (at -5.08 8.89 0))
      (property "Footprint" "" (at 3.81 -1.27 0))
      (property "Datasheet" " ~" (at 3.81 -1.27 0))
      (property "ki_keywords" "connector USB" (at 0 0 0))
      (property "ki_description" "USB Type A connector" (at 0 0 0))
      (property "ki_fp_filters" "USB*" (at 0 0 0))
      (symbol "USB_A_0_1"
        (rectangle (start -5.08 -7.62) (end 5.08 7.62)
          (fill (type background))
        )
        (circle (center -3.81 2.159) (radius 0.635)
          (fill (type outline))
        )
        (rectangle (start -1.524 4.826) (end -4.318 5.334)
          (fill (type outline))
        )
        (rectangle (start -1.27 4.572) (end -4.572 5.842)
          (fill (type none))
        )
        (circle (center -0.635 3.429) (radius 0.381)
          (fill (type outline))
        )
        (rectangle (start -0.127 -7.62) (end 0.127 -6.858)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.175 2.159)
            (xy -2.54 2.159)
            (xy -1.27 3.429)
            (xy -0.635 3.429)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 2.159)
            (xy -1.905 2.159)
            (xy -1.27 0.889)
            (xy 0 0.889)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 2.794)
            (xy 0.635 1.524)
            (xy 1.905 2.159)
            (xy 0.635 2.794)
          )
          (fill (type outline))
        )
        (rectangle (start 0.254 1.27) (end -0.508 0.508)
          (fill (type outline))
        )
        (rectangle (start 5.08 -2.667) (end 4.318 -2.413)
          (fill (type none))
        )
        (rectangle (start 5.08 -0.127) (end 4.318 0.127)
          (fill (type none))
        )
        (rectangle (start 5.08 4.953) (end 4.318 5.207)
          (fill (type none))
        )
      )
      (symbol "USB_A_1_1"
        (polyline
          (pts
            (xy -1.905 2.159)
            (xy 0.635 2.159)
          )
          (fill (type none))
        )
        (pin power_in line (at 7.62 5.08 180) (length 2.54)
          (name "VBUS")
          (number "1")
        )
        (pin bidirectional line (at 7.62 -2.54 180) (length 2.54)
          (name "D-")
          (number "2")
        )
        (pin bidirectional line (at 7.62 0 180) (length 2.54)
          (name "D+")
          (number "3")
        )
        (pin power_in line (at 0 -10.16 90) (length 2.54)
          (name "GND")
          (number "4")
        )
        (pin passive line (at -2.54 -10.16 90) (length 2.54)
          (name "Shield")
          (number "5")
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (at 0.635 2.54 0))
      (property "Value" "C" (at 0.635 -2.54 0))
      (property "Footprint" "" (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (at 0 0 0))
      (property "ki_fp_filters" "C_*" (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:C_Polarized_US" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "C" (at 0.635 2.54 0))
      (property "Value" "C_Polarized_US" (at 0.635 -2.54 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (at 0 0 0))
      (property "ki_description" "Polarized capacitor, US symbol" (at 0 0 0))
      (property "ki_fp_filters" "CP_*" (at 0 0 0))
      (symbol "C_Polarized_US_0_1"
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 2.286)
            (xy -0.762 2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 1.778)
            (xy -1.27 2.794)
          )
          (fill (type none))
        )
        (arc (start 2.032 -1.27) (mid 0 -0.5572) (end -2.032 -1.27)
          (fill (type none))
        )
      )
      (symbol "C_Polarized_US_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 3.302)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (at 2.032 0 90))
      (property "Value" "R" (at 0 0 90))
      (property "Footprint" "" (at -1.778 0 90))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "R res resistor" (at 0 0 0))
      (property "ki_description" "Resistor" (at 0 0 0))
      (property "ki_fp_filters" "R_*" (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:R_Potentiometer_Small" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "RV" (at -4.445 0 90))
      (property "Value" "R_Potentiometer_Small" (at -2.54 0 90))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "resistor variable" (at 0 0 0))
      (property "ki_description" "Potentiometer" (at 0 0 0))
      (property "ki_fp_filters" "Potentiometer*" (at 0 0 0))
      (symbol "R_Potentiometer_Small_0_1"
        (polyline
          (pts
            (xy 0.889 0)
            (xy 0.635 0)
            (xy 1.651 0.381)
            (xy 1.651 -0.381)
            (xy 0.635 0)
            (xy 0.889 0)
          )
          (fill (type outline))
        )
        (rectangle (start 0.762 1.8034) (end -0.762 -1.8034)
          (fill (type none))
        )
      )
      (symbol "R_Potentiometer_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 0.635)
          (name "1")
          (number "1")
        )
        (pin passive line (at 2.54 0 180) (length 0.9906)
          (name "2")
          (number "2")
        )
        (pin passive line (at 0 -2.54 90) (length 0.635)
          (name "3")
          (number "3")
        )
      )
    )
    (symbol "Regulator_Switching:R-78E5.0-1.0" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (at -3.81 3.175 0))
      (property "Value" "R-78E5.0-1.0" (at 0 3.175 0))
      (property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT" (at 1.27 -6.35 0))
      (property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78Exx-1.0.pdf" (at 0 0 0))
      (property "ki_keywords" "dc-dc recom Step-Down DC/DC-Regulator" (at 0 0 0))
      (property "ki_description" "1A Step-Down DC/DC-Regulator, 7-28V input, 5V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, SIP3" (at 0 0 0))
      (property "ki_fp_filters" "Converter*DCDC*RECOM*R*78E*0.5*" (at 0 0 0))
      (symbol "R-78E5.0-1.0_0_1"
        (rectangle (start -5.08 1.905) (end 5.08 -5.08)
          (fill (type background))
        )
      )
      (symbol "R-78E5.0-1.0_1_1"
        (pin power_in line (at -7.62 0 0) (length 2.54)
          (name "IN")
          (number "1")
        )
        (pin power_in line (at 0 -7.62 90) (length 2.54)
          (name "GND")
          (number "2")
        )
        (pin power_out line (at 7.62 0 180) (length 2.54)
          (name "OUT")
          (number "3")
        )
      )
    )
    (symbol "Rovo:NHD-0420HDZ" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at -6.35 19.05 0))
      (property "Value" "NHD-0420DZ" (at 5.08 19.05 0))
      (property "Footprint" "Rovo:NHD-0420DZ" (at 0 -22.86 0))
      (property "Datasheet" "https://newhavendisplay.com/4x20-character-lcd-fstn-display-dz-with-white-side-backlight/" (at 2.54 -2.54 0))
      (property "ki_keywords" "display LCD 20x4" (at 0 0 0))
      (property "ki_description" "LCD 20x4 Alphanumeric 16pin Blue/White/Green Backlight, 8bit parallel" (at 0 0 0))
      (property "ki_fp_filters" "NHD*0420H1Z*" (at 0 0 0))
      (symbol "NHD-0420HDZ_0_1"
        (rectangle (start -7.62 17.78) (end 7.62 -17.78)
          (fill (type background))
        )
      )
      (symbol "NHD-0420HDZ_1_1"
        (pin power_in line (at 0 -20.32 90) (length 2.54)
          (name "VSS")
          (number "1")
        )
        (pin bidirectional line (at -10.16 -5.08 0) (length 2.54)
          (name "DB3")
          (number "10")
        )
        (pin bidirectional line (at -10.16 -7.62 0) (length 2.54)
          (name "DB4")
          (number "11")
        )
        (pin bidirectional line (at -10.16 -10.16 0) (length 2.54)
          (name "DB5")
          (number "12")
        )
        (pin bidirectional line (at -10.16 -12.7 0) (length 2.54)
          (name "DB6")
          (number "13")
        )
        (pin bidirectional line (at -10.16 -15.24 0) (length 2.54)
          (name "DB7")
          (number "14")
        )
        (pin passive line (at 5.08 20.32 270) (length 2.54)
          (name "LED+")
          (number "15")
        )
        (pin passive line (at 5.08 -20.32 90) (length 2.54)
          (name "LED-")
          (number "16")
        )
        (pin power_in line (at 0 20.32 270) (length 2.54)
          (name "VDD")
          (number "2")
        )
        (pin power_in line (at 10.16 8.89 180) (length 2.54)
          (name "VO")
          (number "3")
        )
        (pin input line (at -10.16 15.24 0) (length 2.54)
          (name "RS")
          (number "4")
        )
        (pin input line (at -10.16 12.7 0) (length 2.54)
          (name "R/W")
          (number "5")
        )
        (pin input line (at -10.16 10.16 0) (length 2.54)
          (name "E")
          (number "6")
        )
        (pin bidirectional line (at -10.16 2.54 0) (length 2.54)
          (name "DB0")
          (number "7")
        )
        (pin bidirectional line (at -10.16 0 0) (length 2.54)
          (name "DB1")
          (number "8")
        )
        (pin bidirectional line (at -10.16 -2.54 0) (length 2.54)
          (name "DB2")
          (number "9")
        )
      )
    )
    (symbol "Rovo:Teensy4.1_48_5" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 60.96 0))
      (property "Value" "Teensy4.1" (at 0 58.42 0))
      (property "Footprint" "" (at -10.16 10.16 0))
      (property "Datasheet" "" (at -10.16 10.16 0))
      (symbol "Teensy4.1_48_5_0_0"
        (polyline
          (pts
            (xy -22.86 -6.35)
            (xy 22.86 -6.35)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -17.78 -20.32)
            (xy -17.78 -7.62)
          )
          (fill (type none))
        )
        (text "(250mA max)" (at 11.43 49.53 0))
        (text "(3.6v to 5.5v)" (at 11.43 54.61 0))
        (text "Host" (at -13.97 -13.97 900))
        (text "USB" (at -15.875 -13.97 900))
        (pin bidirectional line (at -27.94 31.75 0) (length 5.08)
          (name "8_TX2_IN1")
          (number "10")
        )
        (pin bidirectional line (at -27.94 29.21 0) (length 5.08)
          (name "9_OUT1C")
          (number "11")
        )
        (pin bidirectional line (at -27.94 26.67 0) (length 5.08)
          (name "10_CS_MQSR")
          (number "12")
        )
        (pin bidirectional line (at -27.94 24.13 0) (length 5.08)
          (name "11_MOSI_CTX1")
          (number "13")
        )
        (pin bidirectional line (at -27.94 21.59 0) (length 5.08)
          (name "12_MISO_MQSL")
          (number "14")
        )
        (pin power_in line (at -27.94 19.05 0) (length 5.08)
          (name "3V3")
          (number "15")
        )
        (pin bidirectional line (at -27.94 16.51 0) (length 5.08)
          (name "24_A10_TX6_SCL2")
          (number "16")
        )
        (pin bidirectional line (at -27.94 13.97 0) (length 5.08)
          (name "25_A11_RX6_SDA2")
          (number "17")
        )
        (pin bidirectional line (at -27.94 11.43 0) (length 5.08)
          (name "26_A12_MOSI1")
          (number "18")
        )
        (pin bidirectional line (at -27.94 8.89 0) (length 5.08)
          (name "27_A13_SCK1")
          (number "19")
        )
        (pin bidirectional line (at -27.94 6.35 0) (length 5.08)
          (name "28_RX7")
          (number "20")
        )
        (pin bidirectional line (at -27.94 3.81 0) (length 5.08)
          (name "29_TX7")
          (number "21")
        )
        (pin bidirectional line (at -27.94 1.27 0) (length 5.08)
          (name "30_CRX3")
          (number "22")
        )
        (pin bidirectional line (at -27.94 -1.27 0) (length 5.08)
          (name "31_CTX3")
          (number "23")
        )
        (pin bidirectional line (at -27.94 -3.81 0) (length 5.08)
          (name "32_OUT1B")
          (number "24")
        )
        (pin bidirectional line (at 27.94 -3.81 180) (length 5.08)
          (name "33_MCLK2")
          (number "25")
        )
        (pin bidirectional line (at 27.94 -1.27 180) (length 5.08)
          (name "34_RX8")
          (number "26")
        )
        (pin bidirectional line (at 27.94 1.27 180) (length 5.08)
          (name "35_TX8")
          (number "27")
        )
        (pin bidirectional line (at 27.94 3.81 180) (length 5.08)
          (name "36_CS")
          (number "28")
        )
        (pin bidirectional line (at 27.94 6.35 180) (length 5.08)
          (name "37_CS")
          (number "29")
        )
        (pin bidirectional line (at 27.94 8.89 180) (length 5.08)
          (name "38_CS1_IN1")
          (number "30")
        )
        (pin bidirectional line (at 27.94 11.43 180) (length 5.08)
          (name "39_MISO1_OUT1A")
          (number "31")
        )
        (pin bidirectional line (at 27.94 13.97 180) (length 5.08)
          (name "40_A16")
          (number "32")
        )
        (pin bidirectional line (at 27.94 16.51 180) (length 5.08)
          (name "41_A17")
          (number "33")
        )
        (pin bidirectional line (at 27.94 21.59 180) (length 5.08)
          (name "13_SCK_LED")
          (number "35")
        )
        (pin bidirectional line (at 27.94 24.13 180) (length 5.08)
          (name "14_A0_TX3_SPDIF_OUT")
          (number "36")
        )
        (pin bidirectional line (at 27.94 26.67 180) (length 5.08)
          (name "15_A1_RX3_SPDIF_IN")
          (number "37")
        )
        (pin bidirectional line (at 27.94 29.21 180) (length 5.08)
          (name "16_A2_RX4_SCL1")
          (number "38")
        )
        (pin bidirectional line (at 27.94 31.75 180) (length 5.08)
          (name "17_A3_TX4_SDA1")
          (number "39")
        )
        (pin bidirectional line (at 27.94 34.29 180) (length 5.08)
          (name "18_A4_SDA")
          (number "40")
        )
        (pin bidirectional line (at 27.94 36.83 180) (length 5.08)
          (name "19_A5_SCL")
          (number "41")
        )
        (pin bidirectional line (at 27.94 39.37 180) (length 5.08)
          (name "20_A6_TX5_LRCLK1")
          (number "42")
        )
        (pin bidirectional line (at 27.94 41.91 180) (length 5.08)
          (name "21_A7_RX5_BCLK1")
          (number "43")
        )
        (pin bidirectional line (at 27.94 44.45 180) (length 5.08)
          (name "22_A8_CTX1")
          (number "44")
        )
        (pin bidirectional line (at 27.94 46.99 180) (length 5.08)
          (name "23_A9_CRX1_MCLK1")
          (number "45")
        )
        (pin output line (at 27.94 49.53 180) (length 5.08)
          (name "3V3")
          (number "46")
        )
        (pin output line (at 27.94 52.07 180) (length 5.08)
          (name "GND")
          (number "47")
        )
        (pin power_in line (at 27.94 54.61 180) (length 5.08)
          (name "VIN")
          (number "48")
        )
        (pin bidirectional line (at -27.94 44.45 0) (length 5.08)
          (name "3_LRCLK2")
          (number "5")
        )
        (pin bidirectional line (at -27.94 41.91 0) (length 5.08)
          (name "4_BCLK2")
          (number "6")
        )
        (pin bidirectional line (at -27.94 39.37 0) (length 5.08)
          (name "5_IN2")
          (number "7")
        )
        (pin bidirectional line (at -27.94 36.83 0) (length 5.08)
          (name "6_OUT1D")
          (number "8")
        )
        (pin bidirectional line (at -27.94 34.29 0) (length 5.08)
          (name "7_RX2_OUT1A")
          (number "9")
        )
      )
      (symbol "Teensy4.1_48_5_0_1"
        (rectangle (start -22.86 57.15) (end 22.86 -21.59)
          (fill (type none))
        )
        (rectangle (start -20.32 -1.27) (end -20.32 -1.27)
          (fill (type none))
        )
      )
      (symbol "Teensy4.1_48_5_1_0"
        (pin power_out line (at -27.94 -8.89 0) (length 5.08)
          (name "5V")
          (number "49")
        )
        (pin bidirectional line (at -27.94 -11.43 0) (length 5.08)
          (name "D-")
          (number "50")
        )
        (pin bidirectional line (at -27.94 -13.97 0) (length 5.08)
          (name "D+")
          (number "51")
        )
        (pin power_in line (at -27.94 -16.51 0) (length 5.08)
          (name "GND")
          (number "52")
        )
        (pin power_in line (at -27.94 -19.05 0) (length 5.08)
          (name "GND")
          (number "53")
        )
      )
      (symbol "Teensy4.1_48_5_1_1"
        (pin power_in line (at -27.94 54.61 0) (length 5.08)
          (name "GND")
          (number "1")
        )
        (pin bidirectional line (at -27.94 52.07 0) (length 5.08)
          (name "0_RX1_CRX2_CS1")
          (number "2")
        )
        (pin bidirectional line (at -27.94 49.53 0) (length 5.08)
          (name "1_TX1_CTX2_MISO1")
          (number "3")
        )
        (pin power_in line (at 27.94 19.05 180) (length 5.08)
          (name "GND")
          (number "34")
        )
        (pin bidirectional line (at -27.94 46.99 0) (length 5.08)
          (name "2_OUT2")
          (number "4")
        )
      )
    )
    (symbol "Rovo:Transformer_Balun_344E" (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "T" (at 0 6.35 0))
      (property "Value" "344E" (at 0 -6.35 0))
      (property "Footprint" "Rovo:Transformer_Balun_344E" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_description" "Transformer, Balun, Video, Simonsen123 344E" (at 0 0 0))
      (symbol "Transformer_Balun_344E_0_1"
        (arc (start -1.524 -3.048) (mid -0.7653 -2.286) (end -1.524 -1.524)
          (fill (type none))
        )
        (arc (start -1.524 -1.524) (mid -0.7653 -0.762) (end -1.524 0)
          (fill (type none))
        )
        (arc (start -1.524 0) (mid -0.7653 0.762) (end -1.524 1.524)
          (fill (type none))
        )
        (arc (start -1.524 1.524) (mid -0.7653 2.286) (end -1.524 3.048)
          (fill (type none))
        )
        (rectangle (start -0.254 3.048) (end 0.254 -3.048)
          (fill (type outline))
        )
        (polyline
          (pts
            (xy -2.54 5.08)
            (xy -1.524 5.08)
            (xy -1.524 3.048)
            (xy -1.524 3.048)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.524 -3.048)
            (xy -1.524 -5.08)
            (xy -2.54 -5.08)
            (xy -2.54 -5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.524 3.048)
            (xy 1.524 5.08)
            (xy 2.54 5.08)
            (xy 2.54 5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -5.08)
            (xy 1.524 -5.08)
            (xy 1.524 -3.048)
            (xy 1.524 -3.048)
          )
          (fill (type none))
        )
        (arc (start 1.524 -1.524) (mid 0.7653 -2.286) (end 1.524 -3.048)
          (fill (type none))
        )
        (arc (start 1.524 0) (mid 0.7653 -0.762) (end 1.524 -1.524)
          (fill (type none))
        )
        (arc (start 1.524 1.524) (mid 0.7653 0.762) (end 1.524 0)
          (fill (type none))
        )
        (arc (start 1.524 3.048) (mid 0.7653 2.286) (end 1.524 1.524)
          (fill (type none))
        )
      )
      (symbol "Transformer_Balun_344E_1_1"
        (pin passive line (at -5.08 5.08 0) (length 2.54)
          (name "VidSig")
          (number "1")
        )
        (pin passive line (at -5.08 -5.08 0) (length 2.54)
          (name "VidRet")
          (number "2")
        )
        (pin passive line (at 5.08 -5.08 180) (length 2.54)
          (name "Vid-")
          (number "3")
        )
        (pin passive line (at 5.08 5.08 180) (length 2.54)
          (name "Vid+")
          (number "4")
        )
      )
    )
    (symbol "dk_Interface-Drivers-Receivers-Transceivers:SN75176BDR" (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (at -3.81 6.35 0))
      (property "Value" "SN75176BDR" (at 2.54 -10.16 0))
      (property "Footprint" "digikey-footprints:SOIC-8_W3.9mm" (at 5.08 5.08 0))
      (property "Datasheet" "http://www.ti.com/general/docs/suppproductinfo.tsp?distId=10&gotoUrl=http%3A%2F%2Fwww.ti.com%2Flit%2Fgpn%2Fsn65176b" (at 5.08 7.62 0))
      (property "Digi-Key_PN" "296-1275-1-ND" (at 5.08 10.16 0))
      (property "MPN" "SN75176BDR" (at 5.08 12.7 0))
      (property "Category" "Integrated Circuits (ICs)" (at 5.08 15.24 0))
      (property "Family" "Interface - Drivers, Receivers, Transceivers" (at 5.08 17.78 0))
      (property "DK_Datasheet_Link" "http://www.ti.com/general/docs/suppproductinfo.tsp?distId=10&gotoUrl=http%3A%2F%2Fwww.ti.com%2Flit%2Fgpn%2Fsn65176b" (at 5.08 20.32 0))
      (property "DK_Detail_Page" "/product-detail/en/texas-instruments/SN75176BDR/296-1275-1-ND/404925" (at 5.08 22.86 0))
      (property "Description" "IC TXRX DIFF BUSS 8SOIC" (at 5.08 25.4 0))
      (property "Manufacturer" "Texas Instruments" (at 5.08 27.94 0))
      (property "Status" "Active" (at 5.08 30.48 0))
      (property "ki_keywords" "296-1275-1-ND" (at 0 0 0))
      (property "ki_description" "IC TXRX DIFF BUSS 8SOIC" (at 0 0 0))
      (symbol "SN75176BDR_0_1"
        (rectangle (start -5.08 5.08) (end 5.08 -7.62)
          (fill (type background))
        )
        (circle (center -1.27 -4.064) (radius 0.254)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 0)
            (xy -2.54 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -5.08)
            (xy -5.08 -5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 1.27)
            (xy -1.27 0.635)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -5.08)
            (xy 1.27 -5.715)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.175 -4.826)
            (xy 3.175 -5.461)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 3.175 0.254)
            (xy 3.175 -0.381)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 3.81 -5.08)
            (xy 3.175 -5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.81 -4.826)
            (xy 3.81 -5.461)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 3.81 0.254)
            (xy 3.81 -0.381)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 5.08 -5.08)
            (xy 4.445 -5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 -2.54)
            (xy -1.27 -2.54)
            (xy -1.27 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 1.27)
            (xy -1.27 2.54)
            (xy -5.08 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0.635)
            (xy 1.905 0.635)
            (xy 1.905 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -5.08)
            (xy 1.27 -0.635)
            (xy 0.635 -0.635)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.175 -4.826)
            (xy 2.54 -5.08)
            (xy 3.175 -5.461)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 3.175 0.254)
            (xy 2.54 0)
            (xy 3.175 -0.381)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 3.81 -4.826)
            (xy 4.445 -5.08)
            (xy 3.81 -5.461)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 3.81 0.254)
            (xy 4.445 0)
            (xy 3.81 -0.381)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy -2.54 1.27)
            (xy -2.54 -1.27)
            (xy 0 0)
            (xy -2.54 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -3.81)
            (xy 0 -6.35)
            (xy -2.54 -5.08)
            (xy 0 -3.81)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -5.08)
            (xy 1.905 -5.08)
            (xy 1.905 -5.715)
            (xy 0.635 -5.715)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.08 0)
            (xy 1.905 0)
            (xy 1.905 -4.445)
            (xy 0 -4.445)
          )
          (fill (type none))
        )
        (circle (center 0.254 -5.715) (radius 0.254)
          (fill (type none))
        )
        (circle (center 0.254 -0.635) (radius 0.254)
          (fill (type none))
        )
        (circle (center 1.27 -5.715) (radius 0.254)
          (fill (type outline))
        )
        (circle (center 1.905 0) (radius 0.254)
          (fill (type outline))
        )
      )
      (symbol "SN75176BDR_1_1"
        (pin output line (at -7.62 -5.08 0) (length 2.54)
          (name "R")
          (number "1")
        )
        (pin input line (at -7.62 -2.54 0) (length 2.54)
          (name "~{RE}")
          (number "2")
        )
        (pin input line (at -7.62 2.54 0) (length 2.54)
          (name "DE")
          (number "3")
        )
        (pin input line (at -7.62 0 0) (length 2.54)
          (name "D")
          (number "4")
        )
        (pin power_in line (at 0 -10.16 90) (length 2.54)
          (name "GND")
          (number "5")
        )
        (pin bidirectional line (at 7.62 0 180) (length 2.54)
          (name "A")
          (number "6")
        )
        (pin bidirectional line (at 7.62 -5.08 180) (length 2.54)
          (name "B")
          (number "7")
        )
        (pin power_in line (at 0 7.62 270) (length 2.54)
          (name "VCC")
          (number "8")
        )
      )
    )
    (symbol "power:+5V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -3.81 0))
      (property "Value" "+5V" (at 0 3.556 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "global power" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+5V\"" (at 0 0 0))
      (symbol "+5V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+5V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+5V")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -6.35 0))
      (property "Value" "GND" (at 0 -3.81 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "global power" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (junction (at 40.64 128.27) (diameter 0) (color 0 0 0 0))
  (junction (at 204.47 101.6) (diameter 0) (color 0 0 0 0))
  (junction (at 157.48 111.76) (diameter 0) (color 0 0 0 0))
  (junction (at 110.49 44.45) (diameter 0) (color 0 0 0 0))
  (junction (at 124.46 31.75) (diameter 0) (color 0 0 0 0))
  (junction (at 45.72 128.27) (diameter 0) (color 0 0 0 0))
  (junction (at 128.27 36.83) (diameter 0) (color 0 0 0 0))
  (junction (at 95.25 149.86) (diameter 0) (color 0 0 0 0))
  (junction (at 161.29 36.83) (diameter 0) (color 0 0 0 0))
  (junction (at 138.43 49.53) (diameter 0) (color 0 0 0 0))
  (junction (at 45.72 83.82) (diameter 0) (color 0 0 0 0))
  (junction (at 171.45 101.6) (diameter 0) (color 0 0 0 0))
  (junction (at 148.59 39.37) (diameter 0) (color 0 0 0 0))
  (junction (at 161.29 44.45) (diameter 0) (color 0 0 0 0))
  (junction (at 124.46 55.88) (diameter 0) (color 0 0 0 0))
  (junction (at 138.43 31.75) (diameter 0) (color 0 0 0 0))
  (junction (at 190.5 109.22) (diameter 0) (color 0 0 0 0))
  (junction (at 161.29 39.37) (diameter 0) (color 0 0 0 0))
  (junction (at 40.64 83.82) (diameter 0) (color 0 0 0 0))
  (junction (at 68.58 154.94) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 29.21 97.79) (xy 35.56 97.79)))
  (wire (pts (xy 128.27 41.91) (xy 130.81 41.91)))
  (wire (pts (xy 55.88 119.38) (xy 67.31 119.38)))
  (wire (pts (xy 161.29 44.45) (xy 161.29 39.37)))
  (wire (pts (xy 78.74 142.24) (xy 78.74 147.32)))
  (wire (pts (xy 171.45 109.22) (xy 190.5 109.22)))
  (wire (pts (xy 76.2 139.7) (xy 95.25 139.7)))
  (wire (pts (xy 161.29 44.45) (xy 161.29 49.53)))
  (wire (pts (xy 95.25 147.32) (xy 95.25 149.86)))
  (wire (pts (xy 146.05 44.45) (xy 161.29 44.45)))
  (wire (pts (xy 120.65 44.45) (xy 130.81 44.45)))
  (wire (pts (xy 222.25 72.39) (xy 222.25 67.31)))
  (wire (pts (xy 82.55 77.47) (xy 82.55 76.2)))
  (wire (pts (xy 138.43 31.75) (xy 151.13 31.75)))
  (wire (pts (xy 198.12 49.53) (xy 184.15 49.53)))
  (wire (pts (xy 148.59 39.37) (xy 151.13 39.37)))
  (wire (pts (xy 45.72 128.27) (xy 45.72 127)))
  (wire (pts (xy 146.05 39.37) (xy 148.59 39.37)))
  (wire (pts (xy 124.46 31.75) (xy 124.46 48.26)))
  (wire (pts (xy 55.88 116.84) (xy 62.23 116.84)))
  (wire (pts (xy 69.85 116.84) (xy 95.25 116.84)))
  (wire (pts (xy 175.26 62.23) (xy 193.04 62.23)))
  (wire (pts (xy 198.12 36.83) (xy 166.37 36.83)))
  (wire (pts (xy 203.2 72.39) (xy 222.25 72.39)))
  (wire (pts (xy 45.72 82.55) (xy 45.72 83.82)))
  (wire (pts (xy 148.59 39.37) (xy 148.59 36.83)))
  (wire (pts (xy 40.64 127) (xy 40.64 128.27)))
  (wire (pts (xy 177.8 34.29) (xy 177.8 72.39)))
  (wire (pts (xy 55.88 91.44) (xy 95.25 91.44)))
  (wire (pts (xy 40.64 83.82) (xy 45.72 83.82)))
  (wire (pts (xy 88.9 39.37) (xy 88.9 81.28)))
  (wire (pts (xy 161.29 36.83) (xy 163.83 36.83)))
  (wire (pts (xy 177.8 72.39) (xy 193.04 72.39)))
  (wire (pts (xy 110.49 55.88) (xy 124.46 55.88)))
  (wire (pts (xy 181.61 46.99) (xy 181.61 81.28)))
  (wire (pts (xy 124.46 31.75) (xy 138.43 31.75)))
  (wire (pts (xy 158.75 31.75) (xy 161.29 31.75)))
  (wire (pts (xy 171.45 101.6) (xy 182.88 101.6)))
  (wire (pts (xy 161.29 39.37) (xy 166.37 39.37)))
  (wire (pts (xy 158.75 39.37) (xy 161.29 39.37)))
  (wire (pts (xy 88.9 39.37) (xy 130.81 39.37)))
  (wire (pts (xy 86.36 83.82) (xy 95.25 83.82)))
  (wire (pts (xy 204.47 101.6) (xy 218.44 101.6)))
  (wire (pts (xy 66.04 154.94) (xy 68.58 154.94)))
  (wire (pts (xy 157.48 135.89) (xy 157.48 111.76)))
  (wire (pts (xy 55.88 121.92) (xy 72.39 121.92)))
  (wire (pts (xy 128.27 36.83) (xy 128.27 41.91)))
  (wire (pts (xy 175.26 31.75) (xy 175.26 62.23)))
  (wire (pts (xy 198.12 101.6) (xy 204.47 101.6)))
  (wire (pts (xy 55.88 93.98) (xy 95.25 93.98)))
  (wire (pts (xy 95.25 142.24) (xy 78.74 142.24)))
  (wire (pts (xy 198.12 34.29) (xy 177.8 34.29)))
  (wire (pts (xy 171.45 39.37) (xy 198.12 39.37)))
  (wire (pts (xy 163.83 44.45) (xy 198.12 44.45)))
  (wire (pts (xy 190.5 109.22) (xy 204.47 109.22)))
  (wire (pts (xy 163.83 36.83) (xy 163.83 44.45)))
  (wire (pts (xy 184.15 49.53) (xy 184.15 86.36)))
  (wire (pts (xy 55.88 114.3) (xy 57.15 114.3)))
  (wire (pts (xy 157.48 111.76) (xy 157.48 78.74)))
  (wire (pts (xy 157.48 78.74) (xy 151.13 78.74)))
  (wire (pts (xy 203.2 62.23) (xy 217.17 62.23)))
  (wire (pts (xy 74.93 119.38) (xy 95.25 119.38)))
  (wire (pts (xy 151.13 111.76) (xy 157.48 111.76)))
  (wire (pts (xy 78.74 147.32) (xy 76.2 147.32)))
  (wire (pts (xy 194.31 41.91) (xy 194.31 52.07)))
  (wire (pts (xy 161.29 49.53) (xy 158.75 49.53)))
  (wire (pts (xy 130.81 36.83) (xy 128.27 36.83)))
  (wire (pts (xy 148.59 36.83) (xy 161.29 36.83)))
  (wire (pts (xy 45.72 128.27) (xy 45.72 129.54)))
  (wire (pts (xy 55.88 96.52) (xy 95.25 96.52)))
  (wire (pts (xy 76.2 144.78) (xy 95.25 144.78)))
  (wire (pts (xy 64.77 114.3) (xy 95.25 114.3)))
  (wire (pts (xy 198.12 41.91) (xy 194.31 41.91)))
  (wire (pts (xy 45.72 83.82) (xy 45.72 86.36)))
  (wire (pts (xy 40.64 83.82) (xy 40.64 86.36)))
  (wire (pts (xy 161.29 31.75) (xy 161.29 36.83)))
  (wire (pts (xy 113.03 44.45) (xy 110.49 44.45)))
  (wire (pts (xy 26.67 128.27) (xy 40.64 128.27)))
  (wire (pts (xy 26.67 83.82) (xy 40.64 83.82)))
  (wire (pts (xy 184.15 86.36) (xy 222.25 86.36)))
  (wire (pts (xy 138.43 49.53) (xy 151.13 49.53)))
  (wire (pts (xy 91.44 44.45) (xy 91.44 78.74)))
  (wire (pts (xy 26.67 91.44) (xy 26.67 95.25)))
  (wire (pts (xy 91.44 78.74) (xy 95.25 78.74)))
  (wire (pts (xy 166.37 36.83) (xy 166.37 39.37)))
  (wire (pts (xy 40.64 128.27) (xy 45.72 128.27)))
  (wire (pts (xy 198.12 46.99) (xy 181.61 46.99)))
  (wire (pts (xy 86.36 36.83) (xy 86.36 83.82)))
  (wire (pts (xy 175.26 31.75) (xy 198.12 31.75)))
  (wire (pts (xy 91.44 44.45) (xy 110.49 44.45)))
  (wire (pts (xy 80.01 121.92) (xy 95.25 121.92)))
  (wire (pts (xy 110.49 44.45) (xy 110.49 48.26)))
  (wire (pts (xy 181.61 81.28) (xy 217.17 81.28)))
  (wire (pts (xy 154.94 76.2) (xy 154.94 74.93)))
  (wire (pts (xy 171.45 39.37) (xy 171.45 101.6)))
  (wire (pts (xy 86.36 36.83) (xy 128.27 36.83)))
  (wire (pts (xy 88.9 81.28) (xy 95.25 81.28)))
  (wire (pts (xy 26.67 100.33) (xy 26.67 128.27)))
  (wire (pts (xy 82.55 76.2) (xy 95.25 76.2)))
  (wire (pts (xy 151.13 76.2) (xy 154.94 76.2)))
  (label "12V" (at 185.42 39.37 0) (fields_autoplaced))
  (label "VID+" (at 185.42 31.75 0) (fields_autoplaced))
  (label "DISP_RW" (at 83.82 93.98 0) (fields_autoplaced))
  (label "USB_D+" (at 82.55 144.78 0) (fields_autoplaced))
  (label "SERB" (at 185.42 36.83 0) (fields_autoplaced))
  (label "DISP_RS" (at 83.82 91.44 0) (fields_autoplaced))
  (label "DISP_D5" (at 83.82 116.84 0) (fields_autoplaced))
  (label "TXD" (at 99.06 39.37 0) (fields_autoplaced))
  (label "AUD+" (at 185.42 46.99 0) (fields_autoplaced))
  (label "DISP_D6" (at 83.82 119.38 0) (fields_autoplaced))
  (label "DISP_E" (at 83.82 96.52 0) (fields_autoplaced))
  (label "USB_VBUS" (at 82.55 139.7 0) (fields_autoplaced))
  (label "RXD" (at 99.06 44.45 0) (fields_autoplaced))
  (label "AUD-" (at 185.42 49.53 0) (fields_autoplaced))
  (label "VID-" (at 185.42 34.29 0) (fields_autoplaced))
  (label "TXE" (at 99.06 36.83 0) (fields_autoplaced))
  (label "DISP_D4" (at 83.82 114.3 0) (fields_autoplaced))
  (label "CONT" (at 30.48 97.79 0) (fields_autoplaced))
  (label "SERA" (at 185.42 44.45 0) (fields_autoplaced))
  (label "VID_RET" (at 208.28 72.39 0) (fields_autoplaced))
  (label "USB_D-" (at 82.55 142.24 0) (fields_autoplaced))
  (label "VID" (at 208.28 62.23 0) (fields_autoplaced))
  (label "DISP_D7" (at 83.82 121.92 0) (fields_autoplaced))
  (label "RXD5" (at 125.73 44.45 0) (fields_autoplaced))
  (symbol (lib_id "Rovo:Transformer_Balun_344E") (at 198.12 67.31 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "T1" (at 198.12 57.15 0))
    (property "Value" "Balun" (at 198.12 59.69 0))
    (property "Footprint" "Rovo:Transformer_Balun_Board" (at 198.12 67.31 0))
    (property "Datasheet" "" (at 198.12 67.31 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (instances
      (project "RVTOP-C"
        (path
          (reference "T1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Connector:Conn_Coaxial") (at 222.25 62.23 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "J2" (at 226.06 61.2532 0))
    (property "Value" "VIDEO" (at 226.06 63.7932 0))
    (property "Footprint" "Rovo:Connector_CUI_RCJ_01_Horizontal" (at 222.25 62.23 0))
    (property "Datasheet" " ~" (at 222.25 62.23 0))
    (pin "1")
    (pin "2")
    (instances
      (project "RVTOP-C"
        (path
          (reference "J2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C_Polarized_US") (at 171.45 105.41 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C3" (at 175.26 104.14 0))
    (property "Value" "470uF25V" (at 175.26 106.045 0))
    (property "Footprint" "Capacitor_THT:CP_Radial_D10.0mm_P3.50mm" (at 171.45 105.41 0))
    (property "Datasheet" "~" (at 171.45 105.41 0))
    (pin "1")
    (pin "2")
    (instances
      (project "RVTOP-C"
        (path
          (reference "C3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 76.2 121.92 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R9" (at 76.2 115.57 90))
    (property "Value" "1K" (at 76.2 118.11 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (at 76.2 123.698 90))
    (property "Datasheet" "~" (at 76.2 121.92 0))
    (pin "1")
    (pin "2")
    (instances
      (project "RVTOP-C"
        (path
          (reference "R9") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+5V") (at 45.72 82.55 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR010" (at 45.72 86.36 0))
    (property "Value" "+5V" (at 45.72 77.47 0))
    (property "Footprint" "" (at 45.72 82.55 0))
    (property "Datasheet" "" (at 45.72 82.55 0))
    (pin "1")
    (instances
      (project "RVTOP-C"
        (path
          (reference "#PWR010") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 68.58 154.94 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR02" (at 68.58 161.29 0))
    (property "Value" "GND" (at 68.58 160.02 0))
    (property "Footprint" "" (at 68.58 154.94 0))
    (property "Datasheet" "" (at 68.58 154.94 0))
    (pin "1")
    (instances
      (project "RVTOP-C"
        (path
          (reference "#PWR02") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 71.12 119.38 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R8" (at 71.12 113.03 90))
    (property "Value" "1K" (at 71.12 115.57 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (at 71.12 121.158 90))
    (property "Datasheet" "~" (at 71.12 119.38 0))
    (pin "1")
    (pin "2")
    (instances
      (project "RVTOP-C"
        (path
          (reference "R8") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 154.94 49.53 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R5" (at 153.67 46.99 90))
    (property "Value" "10K" (at 157.48 46.99 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (at 154.94 51.308 90))
    (property "Datasheet" "~" (at 154.94 49.53 0))
    (pin "1")
    (pin "2")
    (instances
      (project "RVTOP-C"
        (path
          (reference "R5") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 26.67 87.63 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R10" (at 29.21 86.36 0))
    (property "Value" "2K" (at 29.21 88.9 0))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (at 24.892 87.63 90))
    (property "Datasheet" "~" (at 26.67 87.63 0))
    (pin "1")
    (pin "2")
    (instances
      (project "RVTOP-C"
        (path
          (reference "R10") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 138.43 49.53 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR026" (at 138.43 55.88 0))
    (property "Value" "GND" (at 138.43 54.61 0))
    (property "Footprint" "" (at 138.43 49.53 0))
    (property "Datasheet" "" (at 138.43 49.53 0))
    (pin "1")
    (instances
      (project "RVTOP-C"
        (path
          (reference "#PWR026") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 60.96 114.3 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R6" (at 60.96 107.95 90))
    (property "Value" "1K" (at 60.96 110.49 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (at 60.96 116.078 90))
    (property "Datasheet" "~" (at 60.96 114.3 0))
    (pin "1")
    (pin "2")
    (instances
      (project "RVTOP-C"
        (path
          (reference "R6") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Rovo:Teensy4.1_48_5") (at 123.19 130.81 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "M2" (at 123.19 68.58 0))
    (property "Value" "Teensy4.1" (at 123.19 71.12 0))
    (property "Footprint" "Rovo:Teensy41_48_5" (at 113.03 120.65 0))
    (property "Datasheet" "" (at 113.03 120.65 0))
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "30")
    (pin "31")
    (pin "32")
    (pin "33")
    (pin "35")
    (pin "36")
    (pin "37")
    (pin "38")
    (pin "39")
    (pin "40")
    (pin "41")
    (pin "42")
    (pin "43")
    (pin "44")
    (pin "45")
    (pin "46")
    (pin "47")
    (pin "48")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "49")
    (pin "50")
    (pin "51")
    (pin "52")
    (pin "53")
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "34")
    (pin "4")
    (instances
      (project "RVTOP-C"
        (path
          (reference "M2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Connector:USB_A") (at 68.58 144.78 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "J1" (at 68.58 132.08 0))
    (property "Value" "Gamepad" (at 68.58 134.62 0))
    (property "Footprint" "Connector_USB:USB_A_Molex_67643_Horizontal" (at 72.39 146.05 0))
    (property "Datasheet" " ~" (at 72.39 146.05 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (instances
      (project "RVTOP-C"
        (path
          (reference "J1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C_Polarized_US") (at 204.47 105.41 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C4" (at 208.28 104.14 0))
    (property "Value" "470uF25V" (at 208.28 106.045 0))
    (property "Footprint" "Capacitor_THT:CP_Radial_D10.0mm_P3.50mm" (at 204.47 105.41 0))
    (property "Datasheet" "~" (at 204.47 105.41 0))
    (pin "1")
    (pin "2")
    (instances
      (project "RVTOP-C"
        (path
          (reference "C4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 194.31 52.07 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR07" (at 194.31 58.42 0))
    (property "Value" "GND" (at 194.31 57.15 0))
    (property "Footprint" "" (at 194.31 52.07 0))
    (property "Datasheet" "" (at 194.31 52.07 0))
    (pin "1")
    (instances
      (project "RVTOP-C"
        (path
          (reference "#PWR07") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 190.5 109.22 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR09" (at 190.5 115.57 0))
    (property "Value" "GND" (at 190.5 114.3 0))
    (property "Footprint" "" (at 190.5 109.22 0))
    (property "Datasheet" "" (at 190.5 109.22 0))
    (pin "1")
    (instances
      (project "RVTOP-C"
        (path
          (reference "#PWR09") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+5V") (at 124.46 31.75 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR017" (at 124.46 35.56 0))
    (property "Value" "+5V" (at 124.46 26.67 0))
    (property "Footprint" "" (at 124.46 31.75 0))
    (property "Datasheet" "" (at 124.46 31.75 0))
    (pin "1")
    (instances
      (project "RVTOP-C"
        (path
          (reference "#PWR017") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Rovo:NHD-0420HDZ") (at 45.72 106.68 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "M1" (at 44.45 97.79 0))
    (property "Value" "NHD-0420DZ" (at 45.72 100.33 0))
    (property "Footprint" "Rovo:NHD_0420DZ" (at 45.72 129.54 0))
    (property "Datasheet" "https://newhavendisplay.com/4x20-character-lcd-fstn-display-dz-with-white-side-backlight/" (at 43.18 109.22 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (instances
      (project "RVTOP-C"
        (path
          (reference "M1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Regulator_Switching:R-78E5.0-1.0") (at 190.5 101.6 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U4" (at 190.5 95.25 0))
    (property "Value" "R-78E5.0-1.0" (at 190.5 97.79 0))
    (property "Footprint" "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT" (at 191.77 107.95 0))
    (property "Datasheet" "https://www.recom-power.com/pdf/Innoline/R-78Exx-1.0.pdf" (at 190.5 101.6 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (instances
      (project "RVTOP-C"
        (path
          (reference "U4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 154.94 39.37 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R1" (at 151.13 35.56 90))
    (property "Value" "100Ohm" (at 157.48 35.56 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (at 154.94 41.148 90))
    (property "Datasheet" "~" (at 154.94 39.37 0))
    (pin "1")
    (pin "2")
    (instances
      (project "RVTOP-C"
        (path
          (reference "R1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 95.25 149.86 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR04" (at 95.25 156.21 0))
    (property "Value" "GND" (at 95.25 154.94 0))
    (property "Footprint" "" (at 95.25 149.86 0))
    (property "Datasheet" "" (at 95.25 149.86 0))
    (pin "1")
    (instances
      (project "RVTOP-C"
        (path
          (reference "#PWR04") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 110.49 52.07 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R3" (at 113.03 50.8 0))
    (property "Value" "2K" (at 113.03 53.34 0))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (at 108.712 52.07 90))
    (property "Datasheet" "~" (at 110.49 52.07 0))
    (pin "1")
    (pin "2")
    (instances
      (project "RVTOP-C"
        (path
          (reference "R3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 157.48 135.89 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR01" (at 157.48 142.24 0))
    (property "Value" "GND" (at 157.48 140.97 0))
    (property "Footprint" "" (at 157.48 135.89 0))
    (property "Datasheet" "" (at 157.48 135.89 0))
    (pin "1")
    (instances
      (project "RVTOP-C"
        (path
          (reference "#PWR01") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+5V") (at 154.94 74.93 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR016" (at 154.94 78.74 0))
    (property "Value" "+5V" (at 154.94 69.85 0))
    (property "Footprint" "" (at 154.94 74.93 0))
    (property "Datasheet" "" (at 154.94 74.93 0))
    (pin "1")
    (instances
      (project "RVTOP-C"
        (path
          (reference "#PWR016") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Connector:8P8C") (at 208.28 39.37 180) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "J4" (at 217.17 39.37 0))
    (property "Value" "Tether" (at 217.17 41.91 0))
    (property "Footprint" "Connector_RJ:RJ45_Amphenol_54602-x08_Horizontal" (at 208.28 40.005 90))
    (property "Datasheet" "~" (at 208.28 40.005 90))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (instances
      (project "RVTOP-C"
        (path
          (reference "J4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 124.46 52.07 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "C1" (at 128.27 50.8 0))
    (property "Value" "0.1uF_50V_X7R_Rad" (at 128.27 53.34 0))
    (property "Footprint" "Capacitor_THT:C_Rect_L4.6mm_W2.0mm_P2.50mm_MKS02_FKP02" (at 125.4252 55.88 0))
    (property "Datasheet" "~" (at 124.46 52.07 0))
    (pin "1")
    (pin "2")
    (instances
      (project "RVTOP-C"
        (path
          (reference "C1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Connector:Conn_Coaxial") (at 222.25 81.28 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "J3" (at 226.06 80.3032 0))
    (property "Value" "AUDIO" (at 226.06 82.8432 0))
    (property "Footprint" "Rovo:Connector_CUI_RCJ_01_Horizontal" (at 222.25 81.28 0))
    (property "Datasheet" " ~" (at 222.25 81.28 0))
    (pin "1")
    (pin "2")
    (instances
      (project "RVTOP-C"
        (path
          (reference "J3") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 116.84 44.45 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R2" (at 115.57 41.91 90))
    (property "Value" "1K" (at 119.38 41.91 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (at 116.84 46.228 90))
    (property "Datasheet" "~" (at 116.84 44.45 0))
    (pin "1")
    (pin "2")
    (instances
      (project "RVTOP-C"
        (path
          (reference "R2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 82.55 77.47 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR05" (at 82.55 83.82 0))
    (property "Value" "GND" (at 82.55 82.55 0))
    (property "Footprint" "" (at 82.55 77.47 0))
    (property "Datasheet" "" (at 82.55 77.47 0))
    (pin "1")
    (instances
      (project "RVTOP-C"
        (path
          (reference "#PWR05") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 66.04 116.84 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "R7" (at 66.04 110.49 90))
    (property "Value" "1K" (at 66.04 113.03 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (at 66.04 118.618 90))
    (property "Datasheet" "~" (at 66.04 116.84 0))
    (pin "1")
    (pin "2")
    (instances
      (project "RVTOP-C"
        (path
          (reference "R7") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:+5V") (at 218.44 101.6 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR015" (at 214.63 101.6 0))
    (property "Value" "+5V" (at 222.25 101.6 90))
    (property "Footprint" "" (at 218.44 101.6 0))
    (property "Datasheet" "" (at 218.44 101.6 0))
    (pin "1")
    (instances
      (project "RVTOP-C"
        (path
          (reference "#PWR015") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "dk_Interface-Drivers-Receivers-Transceivers:SN75176BDR") (at 138.43 39.37 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "U2" (at 137.16 26.67 0))
    (property "Value" "SN65HVD485EP" (at 132.08 29.21 0))
    (property "Footprint" "Package_DIP:DIP-8_W7.62mm" (at 143.51 34.29 0))
    (property "Datasheet" "" (at 143.51 31.75 0))
    (property "Digi-Key_PN" "296-17498-5-ND" (at 143.51 29.21 0))
    (property "MPN" "SN65HVD485EP" (at 143.51 26.67 0))
    (property "Category" "Integrated Circuits (ICs)" (at 143.51 24.13 0))
    (property "Family" "Interface - Drivers, Receivers, Transceivers" (at 143.51 21.59 0))
    (property "DK_Datasheet_Link" "http://www.ti.com/general/docs/suppproductinfo.tsp?distId=10&gotoUrl=http%3A%2F%2Fwww.ti.com%2Flit%2Fgpn%2Fsn65176b" (at 143.51 19.05 0))
    (property "DK_Detail_Page" "/product-detail/en/texas-instruments/SN75176BDR/296-1275-1-ND/404925" (at 143.51 16.51 0))
    (property "Description" "IC TXRX DIFF BUSS 8SOIC" (at 143.51 13.97 0))
    (property "Manufacturer" "Texas Instruments" (at 143.51 11.43 0))
    (property "Status" "Active" (at 143.51 8.89 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (instances
      (project "RVTOP-C"
        (path
          (reference "U2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R_Potentiometer_Small") (at 26.67 97.79 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "RV1" (at 24.13 96.52 0))
    (property "Value" "1K" (at 24.13 99.06 0))
    (property "Footprint" "Potentiometer_THT:Potentiometer_Bourns_3386X_Horizontal" (at 26.67 97.79 0))
    (property "Datasheet" "~" (at 26.67 97.79 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (instances
      (project "RVTOP-C"
        (path
          (reference "RV1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 124.46 55.88 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR03" (at 124.46 62.23 0))
    (property "Value" "GND" (at 124.46 60.96 0))
    (property "Footprint" "" (at 124.46 55.88 0))
    (property "Datasheet" "" (at 124.46 55.88 0))
    (pin "1")
    (instances
      (project "RVTOP-C"
        (path
          (reference "#PWR03") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Device:R") (at 154.94 31.75 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R4" (at 153.67 29.21 90))
    (property "Value" "10K" (at 157.48 29.21 90))
    (property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (at 154.94 33.528 90))
    (property "Datasheet" "~" (at 154.94 31.75 0))
    (pin "1")
    (pin "2")
    (instances
      (project "RVTOP-C"
        (path
          (reference "R4") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 45.72 129.54 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR08" (at 45.72 135.89 0))
    (property "Value" "GND" (at 45.72 134.62 0))
    (property "Footprint" "" (at 45.72 129.54 0))
    (property "Datasheet" "" (at 45.72 129.54 0))
    (pin "1")
    (instances
      (project "RVTOP-C"
        (path
          (reference "#PWR08") (unit 1)
        )
      )
    )
  )
  (sheet_instances
    (path (page "1"))
  )
)
